<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="154.94" y2="0" width="0" layer="20"/>
<wire x1="154.94" y1="0" x2="154.94" y2="88.9" width="0" layer="20"/>
<wire x1="154.94" y1="88.9" x2="0" y2="88.9" width="0" layer="20"/>
<wire x1="0" y1="88.9" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="stm32f405stamp">
<packages>
<package name="405STAMP">
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="D/7343-31W">
<description>&lt;b&gt;Chip Capacitor Type KEMET D / EIA 7343-21&lt;/b&gt;&lt;p&gt;
KEMET V / EIA 7343-20, KEMET X / EIA 7343-43 Wafe solder</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="E3,5-8">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 3.5 mm, diameter 8 mm</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="PANASONIC_F">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package F&lt;/b&gt;</description>
</package>
<package name="L3225P">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;&lt;p&gt;
precision wire wound</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="diode">
<packages>
<package name="SOT23">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="cds">
<packages>
<package name="SO08">
</package>
<package name="BOURNS3144G">
</package>
<package name="TPAD1.5">
</package>
<package name="AT224A">
</package>
<package name="SOT23-5">
</package>
<package name="TPAD1.3">
</package>
<package name="TPAD1.0">
</package>
<package name="SOT23">
</package>
<package name="VSSOP08">
</package>
<package name="SO08_208">
</package>
<package name="SI08EP">
</package>
<package name="IND_NR604">
</package>
</packages>
</library>
<library name="pot">
<description>&lt;b&gt;Potentiometers&lt;/b&gt;&lt;p&gt;
Beckman, Copal, Piher, Spectrol, Schukat&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B64Y">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Beckman Helitrim 64</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="JP2">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
<package name="JP1">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="magtouch">
<packages>
<package name="SD-MMC_SOCKET-PP">
</package>
</packages>
</library>
<library name="transistor-small-signal">
<description>&lt;b&gt;Small Signal Transistors&lt;/b&gt;&lt;p&gt;
Packages from :&lt;br&gt;
www.infineon.com; &lt;br&gt;
www.semiconductors.com;&lt;br&gt;
www.irf.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="optocoupler">
<description>&lt;b&gt;Opto Couplers&lt;/b&gt;&lt;p&gt;
Siemens, Hewlett-Packard, Texas Instuments, Sharp, Motorola&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL6-04">
<description>&lt;b&gt;DIL 6 0.4 Inch&lt;/b&gt;&lt;p&gt;
Source: http://www.fairchildsemi.com/pf/4N/4N35-M.html</description>
</package>
</packages>
</library>
<library name="cdsrf">
<packages>
<package name="QUEC18">
</package>
<package name="UFL">
</package>
</packages>
</library>
<library name="battery">
<description>&lt;b&gt;Lithium Batteries and NC Accus&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="CH291-1220LF">
<description>&lt;b&gt;Battery Holder, SMT, 12mm&lt;/b&gt;&lt;p&gt;
multicomp PART NO. CH291-1220LF&lt;br&gt;
Source: &lt;a href="http://www.farnell.com/datasheets/1505860.pdf"&gt; Data sheet &lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="_RoweTel">
<packages>
<package name="SM-LP-5001">
</package>
</packages>
</library>
<library name="Arduino-clone">
<description>Arduino Clone pinheaders
By cl@xganon.com
http://www.xganon.com</description>
<packages>
<package name="ESP8266CDSR">
</package>
</packages>
</library>
<library name="con-molex-micro-fit-3_0">
<description>&lt;b&gt;Molex  Micro-Fit 3.0TM Interconnect System&lt;/b&gt;
&lt;p&gt;The Micro-Fit 3.0 is a unique interconnect system designed to meet the need for a high contact density signal or power connector and incorporates many of the features previously found on larger power connectors. These 3.00mm (.118") pitch connectors are the perfect choice when you need compact connectors that carry up to 5 amperes of current. Micro-Fit products are available in circuit sizes 2 to 24 for single and dual row, wire-to-board and wire-to-wire applications. The product family has over 500 part numbers, with many retention choices including fitting nails, solderable clips, and offset terminal retention.

&lt;p&gt;The Micro-Fit 3.0 CPI? and Micro-Fit 3.0 BMI? CPI are compliant pin interface vertical header product extensions to this well known Micro-Fit family. These products are designed for high-density applications which require press-fit headers. The CPI products are appropriate for both power and signal uses as they can carry up to 5 amperes per circuit.

&lt;p&gt;Micro-Fit 3.0 Overmolded Cable Assemblies are available in multiple circuit sizes and cable lengths, featuring a rugged strain relief for signal and power applications. For other cable assembly options, contact harness@molex.com.
&lt;p&gt;Available configurations:
&lt;ul&gt;
&lt;li&gt;Wire to Wire
&lt;li&gt;Wire to Board
&lt;li&gt;BMI (blind mating interface) Wire to Wire Configuration
&lt;li&gt;BMI (blind mating interface) Wire to Board Configuration
&lt;li&gt;BMI (blind mating interface) Board to Board Configuration
&lt;/ul&gt;

&lt;author&gt;Created by divashin@gmail.com&lt;/author&gt;&lt;p&gt;
&lt;p&gt;

&lt;p&gt;Documentation: &lt;u&gt;http://www.molex.com/molex/common/staticLoader.jsp?fileName=/cmc_upload/0/000/0-8/368/full-matrix.html&amp;pageTitle=Micro-Fit,%203.0&amp;chanName=family&amp;frellink=Introduction&amp;familyOID=-8368&amp;channel=Products&amp;oid=-8368&lt;/u&gt;&lt;p&gt;</description>
<packages>
<package name="43045-0400">
<description>Molex Micro-Fit 3.0 - Header Shrouded, Thru hole, Right Angle;  P/N: SD-43045-0400, SD-43045-0401, SD-43045-0402

&lt;p&gt;&lt;a href ='http://www.molex.com/pdm_docs/sd/430450200_sd.pdf'&gt;http://www.molex.com/pdm_docs/sd/430450200_sd.pdf&lt;/a&gt;</description>
</package>
<package name="43045-0600">
<description>Molex Micro-Fit 3.0 - Header Shrouded, Thru hole, Right Angle;  P/N: SD-43045-0600, SD-43045-0601, SD-43045-0602

&lt;p&gt;&lt;a href ='http://www.molex.com/pdm_docs/sd/430450200_sd.pdf'&gt;http://www.molex.com/pdm_docs/sd/430450200_sd.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="stm32f405stamp" package="405STAMP" value="405STAMP">
<attribute name="NAME"/>
</element>
<element name="C8" library="rcl" package="D/7343-31W" value="47uF"/>
<element name="OUT" library="cds" package="TPAD1.3" value="TPAD1.3MM">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="rcl" package="E3,5-8" value="100uF"/>
<element name="U2" library="cds" package="SO08" value="LM386">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R2" library="cds" package="BOURNS3144G" value="100k">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C2" library="rcl" package="C0603" value="22nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="rcl" package="C0603" value="22nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="rcl" package="R0603" value="10R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="rcl" package="C0603" value="100nf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="rcl" package="C0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl" package="R0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="rcl" package="C0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="rcl" package="C0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="rcl" package="PANASONIC_F" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUT1" library="cds" package="TPAD1.5" value="TPAD1.5MM">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="+12V" library="cds" package="TPAD1.3" value="TPAD1.3MM">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="rcl" package="C0603" value="1nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="rcl" package="E3,5-8" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="R1206" value="4R7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FB1" library="rcl" package="L3225P" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="rcl" package="C0603" value="1nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="cds" package="SO08" value="MCP602S">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="IC3" library="cds" package="SO08" value="MCP602S">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R6" library="rcl" package="R0603" value="22k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="rcl" package="R0603" value="22k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="rcl" package="R0603" value="22k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="rcl" package="R0603" value="5k1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="rcl" package="C0603" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="rcl" package="R0603" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="rcl" package="R0603" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="rcl" package="R0603" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="rcl" package="C0603" value="1nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="rcl" package="C0603" value="39nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="pot" package="B64Y" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="rcl" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="rcl" package="R0603" value="5k1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="rcl" package="C0603" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="rcl" package="R0603" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="rcl" package="R0603" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="rcl" package="C0603" value="1nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="rcl" package="C0603" value="39nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="pot" package="B64Y" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="rcl" package="C0603" value="2u2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="rcl" package="C0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="rcl" package="C0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T1" library="cds" package="AT224A" value="TCA-1T1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T2" library="cds" package="AT224A" value="TCA-1T1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="jumper" package="JP2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="jumper" package="JP2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="pot" package="B64Y" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="rcl" package="C0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C28" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C29" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FB2" library="rcl" package="L3225P" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="cds" package="SOT23-5" value="AS321">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C30" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="rcl" package="R0603" value="10R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="rcl" package="C1206" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FB3" library="rcl" package="L3225P" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FB4" library="rcl" package="L3225P" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FB5" library="rcl" package="L3225P" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FB6" library="rcl" package="L3225P" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C31" library="rcl" package="C0603" value="1nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C32" library="rcl" package="C0603" value="1nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND" library="cds" package="TPAD1.3" value="TPAD1.3MM">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="cds" package="SOT23-5" value="AS321">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C33" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="rcl" package="R0603" value="10R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C34" library="rcl" package="C0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="rcl" package="R0603" value="100R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C35" library="rcl" package="C0603" value="1nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="rcl" package="R0603" value="2k2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="rcl" package="R0603" value="22k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="rcl" package="R0603" value="22k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C36" library="rcl" package="C0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C37" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="rcl" package="R0603" value="2k2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="rcl" package="R0603" value="2k2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C38" library="rcl" package="C0603" value="220nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="pot" package="B64Y" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="rcl" package="R0603" value="1k5">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C39" library="rcl" package="C0603" value="100pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U7" library="magtouch" package="SD-MMC_SOCKET-PP" value="SD">
<attribute name="NAME"/>
</element>
<element name="C40" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C41" library="rcl" package="C0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3T_CON" library="cds" package="TPAD1.0" value="TPAD1.0MM"/>
<element name="U3R_CON" library="cds" package="TPAD1.0" value="TPAD1.0MM"/>
<element name="Q3" library="transistor-small-signal" package="SOT23" value="BSS84">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="rcl" package="R0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U5" library="cds" package="SO08" value="75176">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="T8" library="cds" package="SOT23" value="PMBT2907">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="rcl" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R34" library="rcl" package="R0603" value="22k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C42" library="rcl" package="C0603" value="1n5">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C43" library="rcl" package="C1206" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R35" library="rcl" package="R0805" value="120R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R36" library="rcl" package="R0603" value="10R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R37" library="rcl" package="R0603" value="10R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="jumper" package="JP1" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U8" library="cds" package="VSSOP08" value="TXB0102">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C44" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C45" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2TX" library="cds" package="TPAD1.0" value="TPAD1.0MM"/>
<element name="U4RX" library="cds" package="TPAD1.0" value="TPAD1.0MM"/>
<element name="U4TX" library="cds" package="TPAD1.0" value="TPAD1.0MM"/>
<element name="U2RX" library="cds" package="TPAD1.0" value="TPAD1.0MM"/>
<element name="S1" library="optocoupler" package="DIL6-04" value="4N26TM">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R38" library="rcl" package="R0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FB7" library="rcl" package="L3225P" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FB8" library="rcl" package="L3225P" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="transistor-small-signal" package="SOT23" value="BSS84">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R39" library="rcl" package="R0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C46" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C47" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="diode" package="SOT23" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C48" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="rcl" package="R1206" value="47nH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U6" library="cdsrf" package="QUEC18" value="QUECTEL70">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R40" library="rcl" package="R0603" value="10R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="B2" library="battery" package="CH291-1220LF" value="B1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P2" library="cdsrf" package="UFL" value="U.FL">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T1A" library="_RoweTel" package="SM-LP-5001" value="SM-LP-5001">
<attribute name="NAME"/>
</element>
<element name="T2A" library="_RoweTel" package="SM-LP-5001" value="SM-LP-5001">
<attribute name="NAME"/>
</element>
<element name="IC5" library="cds" package="SO08_208" value="W25Q_FLASH">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R41" library="rcl" package="R0603" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R42" library="rcl" package="R0603" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C49" library="rcl" package="C0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C50" library="rcl" package="C0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C51" library="rcl" package="C0805" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C52" library="rcl" package="C0805" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R43" library="rcl" package="R0603" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R44" library="rcl" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U9" library="cds" package="SI08EP" value="RT8284">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R45" library="rcl" package="R0603" value="26k1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C53" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C54" library="rcl" package="C0603" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C55" library="rcl" package="C0603" value="nofit">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C56" library="rcl" package="C0603" value="3n3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R46" library="rcl" package="R0603" value="13k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="cds" package="IND_NR604" value="10uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="rcl" package="R0603" value="26k1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U10" library="Arduino-clone" package="ESP8266CDSR" value="ESP8266CDS"/>
<element name="X2" library="con-molex-micro-fit-3_0" package="43045-0400" value="">
<attribute name="MATERIAL" value=""/>
</element>
<element name="P3" library="con-molex-micro-fit-3_0" package="43045-0600" value=""/>
</elements>
<signals>
<signal name="0V">
<contactref element="C1" pad="-"/>
<contactref element="C8" pad="-"/>
<contactref element="U1" pad="30"/>
<contactref element="U1" pad="55"/>
<contactref element="U1" pad="29"/>
<contactref element="U1" pad="1"/>
<contactref element="U2" pad="4"/>
<contactref element="U2" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C15" pad="-"/>
<contactref element="C16" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="C21" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="R16" pad="1"/>
<contactref element="C24" pad="2"/>
<contactref element="C25" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="T1" pad="1"/>
<contactref element="T2" pad="4"/>
<contactref element="R21" pad="A"/>
<contactref element="C28" pad="2"/>
<contactref element="C29" pad="2"/>
<contactref element="U3" pad="2"/>
<contactref element="C30" pad="2"/>
<contactref element="R22" pad="1"/>
<contactref element="C19" pad="2"/>
<contactref element="IC2" pad="4"/>
<contactref element="IC3" pad="4"/>
<contactref element="GND" pad="1"/>
<contactref element="C33" pad="2"/>
<contactref element="U4" pad="2"/>
<contactref element="C34" pad="2"/>
<contactref element="R26" pad="2"/>
<contactref element="C36" pad="2"/>
<contactref element="C37" pad="2"/>
<contactref element="C35" pad="2"/>
<contactref element="U7" pad="G4"/>
<contactref element="U7" pad="G3"/>
<contactref element="U7" pad="G2"/>
<contactref element="U7" pad="G1"/>
<contactref element="U7" pad="6"/>
<contactref element="C40" pad="2"/>
<contactref element="C41" pad="2"/>
<contactref element="U5" pad="5"/>
<contactref element="U5" pad="2"/>
<contactref element="R34" pad="1"/>
<contactref element="C42" pad="2"/>
<contactref element="C43" pad="2"/>
<contactref element="U8" pad="2"/>
<contactref element="U8" pad="6"/>
<contactref element="C45" pad="2"/>
<contactref element="C44" pad="2"/>
<contactref element="C46" pad="2"/>
<contactref element="U6" pad="1"/>
<contactref element="U6" pad="10"/>
<contactref element="U6" pad="12"/>
<contactref element="B2" pad="-"/>
<contactref element="C48" pad="2"/>
<contactref element="P2" pad="1"/>
<contactref element="P2" pad="2"/>
<contactref element="T1A" pad="1"/>
<contactref element="T2A" pad="4"/>
<contactref element="IC5" pad="4"/>
<contactref element="U9" pad="4"/>
<contactref element="U9" pad="9"/>
<contactref element="R44" pad="1"/>
<contactref element="C52" pad="2"/>
<contactref element="C51" pad="2"/>
<contactref element="C50" pad="2"/>
<contactref element="C49" pad="2"/>
<contactref element="C53" pad="2"/>
<contactref element="C55" pad="2"/>
<contactref element="R46" pad="1"/>
<contactref element="X2" pad="P$4"/>
</signal>
<signal name="+12V">
<contactref element="C1" pad="+"/>
<contactref element="C4" pad="1"/>
<contactref element="+12V" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="U9" pad="2"/>
<contactref element="C50" pad="1"/>
<contactref element="C49" pad="1"/>
<contactref element="R43" pad="1"/>
<contactref element="X2" pad="P$1"/>
</signal>
<signal name="+5V">
<contactref element="OUT" pad="1"/>
<contactref element="C8" pad="+"/>
<contactref element="U1" pad="54"/>
<contactref element="U5" pad="8"/>
<contactref element="T8" pad="2"/>
<contactref element="C43" pad="1"/>
<contactref element="U8" pad="7"/>
<contactref element="C45" pad="1"/>
<contactref element="C52" pad="1"/>
<contactref element="C51" pad="1"/>
<contactref element="R45" pad="2"/>
<contactref element="L2" pad="2"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="+3V3">
<contactref element="U1" pad="53"/>
<contactref element="FB2" pad="1"/>
<contactref element="U3" pad="5"/>
<contactref element="C30" pad="1"/>
<contactref element="R23" pad="2"/>
<contactref element="Q3" pad="2"/>
<contactref element="U8" pad="3"/>
<contactref element="C44" pad="1"/>
<contactref element="S1" pad="1"/>
<contactref element="Q1" pad="2"/>
<contactref element="IC5" pad="8"/>
<contactref element="R41" pad="2"/>
<contactref element="R42" pad="2"/>
</signal>
<signal name="ADC1">
<contactref element="C23" pad="2"/>
<contactref element="IC2" pad="7"/>
<contactref element="IC2" pad="6"/>
<contactref element="U1" pad="36"/>
</signal>
<signal name="ADC2">
<contactref element="R31" pad="1"/>
<contactref element="U1" pad="37"/>
</signal>
<signal name="DAC1">
<contactref element="U1" pad="32"/>
<contactref element="IC3" pad="3"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="DAC2">
<contactref element="U1" pad="33"/>
<contactref element="U3" pad="1"/>
<contactref element="R22" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U2" pad="3"/>
<contactref element="R2" pad="2"/>
<contactref element="C13" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="3"/>
<contactref element="C12" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="U2" pad="5"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="C11" pad="+"/>
</signal>
<signal name="N$5">
<contactref element="U2" pad="8"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="R4" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="R4" pad="1"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U2" pad="7"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="R5" pad="2"/>
<contactref element="C15" pad="+"/>
<contactref element="U2" pad="6"/>
</signal>
<signal name="N$9">
<contactref element="C11" pad="-"/>
<contactref element="FB1" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="OUT1" pad="1"/>
<contactref element="FB1" pad="2"/>
<contactref element="C16" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="R7" pad="1"/>
<contactref element="IC2" pad="3"/>
<contactref element="C17" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="R6" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="C18" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="IC2" pad="2"/>
<contactref element="R15" pad="S"/>
</signal>
<signal name="N$16">
<contactref element="IC2" pad="1"/>
<contactref element="R11" pad="2"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="R10" pad="2"/>
<contactref element="C21" pad="1"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="R14" pad="2"/>
<contactref element="IC2" pad="5"/>
<contactref element="C22" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="C23" pad="1"/>
<contactref element="R13" pad="2"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="R11" pad="1"/>
<contactref element="R15" pad="E"/>
</signal>
<signal name="N$23">
<contactref element="R15" pad="A"/>
<contactref element="C19" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="IC3" pad="1"/>
<contactref element="IC3" pad="2"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="R17" pad="2"/>
<contactref element="C24" pad="1"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="R19" pad="2"/>
<contactref element="C25" pad="1"/>
<contactref element="IC3" pad="5"/>
</signal>
<signal name="N$27">
<contactref element="R18" pad="2"/>
<contactref element="R19" pad="1"/>
<contactref element="C26" pad="1"/>
</signal>
<signal name="A1">
<contactref element="IC3" pad="6"/>
<contactref element="C26" pad="2"/>
<contactref element="IC3" pad="7"/>
<contactref element="C20" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="R20" pad="S"/>
<contactref element="C27" pad="1"/>
</signal>
<signal name="T1_2">
<contactref element="T1" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="T1A" pad="2"/>
</signal>
<signal name="T1_3">
<contactref element="T1" pad="3"/>
<contactref element="JP1" pad="3"/>
<contactref element="T1A" pad="3"/>
</signal>
<signal name="N$31">
<contactref element="JP1" pad="2"/>
<contactref element="C20" pad="2"/>
</signal>
<signal name="T1_4">
<contactref element="T1" pad="4"/>
<contactref element="R20" pad="E"/>
<contactref element="T1A" pad="4"/>
</signal>
<signal name="N$37">
<contactref element="R21" pad="S"/>
<contactref element="C17" pad="2"/>
</signal>
<signal name="N$38">
<contactref element="FB2" pad="2"/>
<contactref element="C28" pad="1"/>
<contactref element="C29" pad="1"/>
<contactref element="R8" pad="2"/>
<contactref element="IC2" pad="8"/>
<contactref element="IC3" pad="8"/>
</signal>
<signal name="N$10">
<contactref element="C12" pad="1"/>
<contactref element="U3" pad="4"/>
<contactref element="U3" pad="3"/>
</signal>
<signal name="N$39">
<contactref element="C27" pad="2"/>
<contactref element="FB4" pad="1"/>
<contactref element="C31" pad="2"/>
</signal>
<signal name="RADTX_HOT">
<contactref element="FB4" pad="2"/>
<contactref element="P3" pad="P$2"/>
</signal>
<signal name="N$40">
<contactref element="JP2" pad="2"/>
<contactref element="FB3" pad="1"/>
<contactref element="C32" pad="1"/>
</signal>
<signal name="T1_6">
<contactref element="T1" pad="6"/>
<contactref element="R20" pad="A"/>
<contactref element="FB6" pad="1"/>
<contactref element="C31" pad="1"/>
<contactref element="T1A" pad="6"/>
</signal>
<signal name="RADTX_RET">
<contactref element="FB6" pad="2"/>
<contactref element="P3" pad="P$5"/>
</signal>
<signal name="IN0">
<contactref element="FB5" pad="2"/>
<contactref element="P3" pad="P$4"/>
</signal>
<signal name="IN1">
<contactref element="FB3" pad="2"/>
<contactref element="P3" pad="P$1"/>
</signal>
<signal name="AV">
<contactref element="R23" pad="1"/>
<contactref element="U4" pad="5"/>
<contactref element="C33" pad="1"/>
<contactref element="C34" pad="1"/>
<contactref element="R25" pad="1"/>
<contactref element="R27" pad="1"/>
</signal>
<signal name="N$32">
<contactref element="R27" pad="2"/>
<contactref element="R26" pad="1"/>
<contactref element="U4" pad="1"/>
<contactref element="C36" pad="1"/>
<contactref element="C37" pad="1"/>
</signal>
<signal name="N$43">
<contactref element="R24" pad="2"/>
<contactref element="R25" pad="2"/>
<contactref element="C35" pad="1"/>
<contactref element="C38" pad="2"/>
</signal>
<signal name="N$44">
<contactref element="U4" pad="3"/>
<contactref element="R28" pad="1"/>
<contactref element="R29" pad="1"/>
</signal>
<signal name="N$45">
<contactref element="R28" pad="2"/>
<contactref element="C38" pad="1"/>
</signal>
<signal name="N$46">
<contactref element="R30" pad="A"/>
<contactref element="R29" pad="2"/>
<contactref element="R30" pad="S"/>
<contactref element="C39" pad="2"/>
</signal>
<signal name="N$48">
<contactref element="R30" pad="E"/>
<contactref element="U4" pad="4"/>
<contactref element="R31" pad="2"/>
<contactref element="C39" pad="1"/>
</signal>
<signal name="N$47">
<contactref element="R24" pad="1"/>
</signal>
<signal name="SPI1_SCK">
<contactref element="U1" pad="9"/>
</signal>
<signal name="SPI1_MISO">
<contactref element="U1" pad="10"/>
</signal>
<signal name="SPI1_MOSI">
<contactref element="U1" pad="11"/>
</signal>
<signal name="SPI1_NSS">
<contactref element="U1" pad="4"/>
</signal>
<signal name="SD2">
<contactref element="U7" pad="1"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="SD3">
<contactref element="U7" pad="2"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="SD_CMD">
<contactref element="U7" pad="3"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="SD_CLK">
<contactref element="U7" pad="5"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="SD0">
<contactref element="U7" pad="7"/>
<contactref element="U1" pad="48"/>
</signal>
<signal name="SD1">
<contactref element="U7" pad="8"/>
<contactref element="U1" pad="49"/>
</signal>
<signal name="SD_SW">
<contactref element="U7" pad="9"/>
<contactref element="U1" pad="50"/>
</signal>
<signal name="U6RX">
<contactref element="U1" pad="47"/>
<contactref element="U6" pad="2"/>
</signal>
<signal name="U6TX">
<contactref element="U1" pad="46"/>
<contactref element="U6" pad="3"/>
</signal>
<signal name="N$53">
<contactref element="U1" pad="40"/>
<contactref element="U3T_CON" pad="1"/>
</signal>
<signal name="N$54">
<contactref element="U1" pad="41"/>
<contactref element="U3R_CON" pad="1"/>
</signal>
<signal name="N$55">
<contactref element="U7" pad="4"/>
<contactref element="C40" pad="1"/>
<contactref element="C41" pad="1"/>
<contactref element="Q3" pad="3"/>
</signal>
<signal name="N$56">
<contactref element="R32" pad="1"/>
<contactref element="Q3" pad="1"/>
</signal>
<signal name="SD_PWR">
<contactref element="R32" pad="2"/>
<contactref element="U1" pad="51"/>
</signal>
<signal name="I2C1SCL">
<contactref element="U1" pad="15"/>
</signal>
<signal name="I2C1SDA">
<contactref element="U1" pad="16"/>
</signal>
<signal name="U1TX">
<contactref element="U1" pad="12"/>
<contactref element="U8" pad="5"/>
</signal>
<signal name="U1RX">
<contactref element="U1" pad="13"/>
<contactref element="U8" pad="4"/>
</signal>
<signal name="TXD">
<contactref element="R35" pad="1"/>
<contactref element="R37" pad="1"/>
<contactref element="X2" pad="P$3"/>
</signal>
<signal name="TXD'">
<contactref element="R36" pad="1"/>
<contactref element="JP3" pad="2"/>
<contactref element="X2" pad="P$2"/>
</signal>
<signal name="N$57">
<contactref element="T8" pad="1"/>
<contactref element="R33" pad="1"/>
</signal>
<signal name="N$58">
<contactref element="R34" pad="2"/>
<contactref element="C42" pad="1"/>
<contactref element="T8" pad="3"/>
<contactref element="U5" pad="3"/>
</signal>
<signal name="N$59">
<contactref element="U5" pad="7"/>
<contactref element="R36" pad="2"/>
</signal>
<signal name="N$60">
<contactref element="U5" pad="6"/>
<contactref element="R37" pad="2"/>
</signal>
<signal name="N$61">
<contactref element="JP3" pad="1"/>
<contactref element="R35" pad="2"/>
</signal>
<signal name="/U1TXD">
<contactref element="U5" pad="4"/>
<contactref element="R33" pad="2"/>
<contactref element="U8" pad="8"/>
</signal>
<signal name="/U1RXD">
<contactref element="U5" pad="1"/>
<contactref element="U8" pad="1"/>
</signal>
<signal name="N$62">
<contactref element="U1" pad="34"/>
</signal>
<signal name="N$63">
<contactref element="U1" pad="35"/>
</signal>
<signal name="U4RX">
<contactref element="U1" pad="27"/>
<contactref element="U4RX" pad="1"/>
</signal>
<signal name="U2TX">
<contactref element="U1" pad="28"/>
<contactref element="U2TX" pad="1"/>
</signal>
<signal name="U4TX">
<contactref element="U1" pad="26"/>
<contactref element="U4TX" pad="1"/>
</signal>
<signal name="U2RX">
<contactref element="U1" pad="31"/>
<contactref element="U2RX" pad="1"/>
</signal>
<signal name="CPTT">
<contactref element="U1" pad="25"/>
<contactref element="R38" pad="1"/>
</signal>
<signal name="N$64">
<contactref element="S1" pad="2"/>
<contactref element="R38" pad="2"/>
</signal>
<signal name="N$65">
<contactref element="S1" pad="4"/>
<contactref element="FB7" pad="1"/>
</signal>
<signal name="N$66">
<contactref element="S1" pad="5"/>
<contactref element="FB8" pad="1"/>
</signal>
<signal name="PTTG">
<contactref element="FB7" pad="2"/>
<contactref element="P3" pad="P$6"/>
</signal>
<signal name="PTTS">
<contactref element="FB8" pad="2"/>
<contactref element="P3" pad="P$3"/>
</signal>
<signal name="N$67">
<contactref element="R39" pad="1"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="GPS_PWR">
<contactref element="R39" pad="2"/>
<contactref element="U1" pad="52"/>
</signal>
<signal name="ANT">
<contactref element="C47" pad="1"/>
<contactref element="L1" pad="1"/>
<contactref element="P2" pad="3"/>
</signal>
<signal name="N$68">
<contactref element="C47" pad="2"/>
<contactref element="U6" pad="11"/>
</signal>
<signal name="N$69">
<contactref element="D2" pad="3"/>
<contactref element="C48" pad="1"/>
<contactref element="U6" pad="6"/>
</signal>
<signal name="N$70">
<contactref element="D2" pad="2"/>
<contactref element="B2" pad="+"/>
</signal>
<signal name="N$71">
<contactref element="R40" pad="1"/>
<contactref element="L1" pad="2"/>
</signal>
<signal name="N$72">
<contactref element="R40" pad="2"/>
<contactref element="U6" pad="14"/>
</signal>
<signal name="N$73">
<contactref element="C46" pad="1"/>
<contactref element="D2" pad="1"/>
<contactref element="U6" pad="8"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="T2_6">
<contactref element="T2A" pad="6"/>
<contactref element="T2" pad="6"/>
<contactref element="R21" pad="E"/>
</signal>
<signal name="T2_3">
<contactref element="T2A" pad="3"/>
<contactref element="FB5" pad="1"/>
<contactref element="T2" pad="3"/>
<contactref element="C32" pad="2"/>
</signal>
<signal name="T2_2">
<contactref element="T2A" pad="2"/>
<contactref element="JP2" pad="3"/>
<contactref element="T2" pad="2"/>
</signal>
<signal name="T2_1">
<contactref element="T2A" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="T2" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="IC5" pad="1"/>
<contactref element="U1" pad="42"/>
</signal>
<signal name="N$30">
<contactref element="IC5" pad="2"/>
<contactref element="U1" pad="44"/>
</signal>
<signal name="N$33">
<contactref element="IC5" pad="5"/>
<contactref element="U1" pad="45"/>
</signal>
<signal name="N$34">
<contactref element="IC5" pad="6"/>
<contactref element="U1" pad="43"/>
</signal>
<signal name="N$35">
<contactref element="IC5" pad="7"/>
<contactref element="R41" pad="1"/>
</signal>
<signal name="N$36">
<contactref element="IC5" pad="3"/>
<contactref element="R42" pad="1"/>
</signal>
<signal name="N$41">
<contactref element="U9" pad="7"/>
<contactref element="R43" pad="2"/>
</signal>
<signal name="N$50">
<contactref element="R45" pad="1"/>
<contactref element="R44" pad="2"/>
<contactref element="U9" pad="5"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$51">
<contactref element="U9" pad="8"/>
<contactref element="C53" pad="1"/>
</signal>
<signal name="N$52">
<contactref element="U9" pad="1"/>
<contactref element="C54" pad="2"/>
</signal>
<signal name="N$74">
<contactref element="U9" pad="6"/>
<contactref element="C55" pad="1"/>
<contactref element="C56" pad="1"/>
</signal>
<signal name="N$75">
<contactref element="U9" pad="3"/>
<contactref element="L2" pad="1"/>
<contactref element="C54" pad="1"/>
</signal>
<signal name="N$76">
<contactref element="R46" pad="2"/>
<contactref element="C56" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
